**Hardware:**

Signal

Conditioning

Sensor 1: Korotkoff Microphone

Sensor 2: Oscillometer

Analog to Digital Converter

Digital Signal Processing

LCD Display

SOFTWARE: A

Pump

& LED

Pump & LED Control